**Cementitious Product EPD**

ASTM. (2016). EPD Ref: EPD 034 for Masonry cement by Portland Cement Association. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2016). EPD Ref: EPD 033 for Blended hydraulic cement by Portland Cement Association. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2016). EPD Ref: EPD 035 for Portland cement by Portland Cement Association. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2015). EPD Ref: EPD-011 for Slag cement by Slag Cement Association. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ATILH. (2017). EPD Ref: CEM I for CEM I by ATILH. Retrieved from https://www.infociments.fr/ciments/ciments-declaration-environnementale-inventaire-analyse-du-cycle-de-vie.

ATILH. (2017). EPD Ref: CEM II/A-L for Average French CEM II/A-L by ATILH. Retrieved from https://www.infociments.fr/ciments/ciments-declaration-environnementale-inventaire-analyse-du-cycle-de-vie.

ATILH. (2017). EPD Ref: CEM II/A-S for Average French CEM II/A-S by ATILH. Retrieved from https://www.infociments.fr/ciments/ciments-declaration-environnementale-inventaire-analyse-du-cycle-de-vie.

ATILH. (2017). EPD Ref: CEM II/B-L or LL for Average French CEM II/B-L or LL by ATILH. Retrieved from https://www.infociments.fr/ciments/ciments-declaration-environnementale-inventaire-analyse-du-cycle-de-vie.

ATILH. (2017). EPD Ref: CEM II/B-M for Average French CEM II/B-M by ATILH. Retrieved from https://www.infociments.fr/ciments/ciments-declaration-environnementale-inventaire-analyse-du-cycle-de-vie.

ATILH. (2017). EPD Ref: CEM III/A for CEM III/A by ATILH. Retrieved from https://www.infociments.fr/ciments/ciments-declaration-environnementale-inventaire-analyse-du-cycle-de-vie.

ATILH. (2017). EPD Ref: CEM III/B for CEM III/B 42.5 by ATILH. Retrieved from https://www.infociments.fr/ciments/ciments-declaration-environnementale-inventaire-analyse-du-cycle-de-vie.

ATILH. (2019). EPD Ref: CEM III/A-PM ES for CEM III/A-PM ES by ATILH. Retrieved from https://www.infociments.fr/ciments/ciments-declaration-environnementale-inventaire-analyse-du-cycle-de-vie.

ATILH. (2019). EPD Ref: CEM III/A (non PM-ES) for CEM III/A non PM ES by ATILH. Retrieved from https://www.infociments.fr/ciments/ciments-declaration-environnementale-inventaire-analyse-du-cycle-de-vie.

ATILH. (2017). EPD Ref: CEM V for Average French CEM V by ATILH. Retrieved from https://www.infociments.fr/ciments/ciments-declaration-environnementale-inventaire-analyse-du-cycle-de-vie.

BCS Oko-Garantie. (2017). EPD Ref: Fly ash - EFA-Füller® S-B/F by BauMineral. Retrieved from https://www.kiwa.com/de/de/veroffentlichte-epds/.

BRE EPD. (2019). EPD Ref: BRE EPD 000242 for CEM I 52.5 by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE EPD. (2019). EPD Ref: BRE EPD 000243 for Hanson CEM II (UK) by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE EPD. (2019). EPD Ref: BRE EPD 000245 for Regen - GGBS by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE EPD. (2019). EPD Ref: BRE EPD 000244 for Hanson CEM II (UK) by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

Cembureau. (2015). EPD Ref: cem for Representative European CEM I by cembureau. Retrieved from https://cembureau.eu/policy-focus/sustainable-construction/#Sustainability\_standards.

Cembureau. (2015). EPD Ref: cemii for Cembureau Average CEM II (EU) by cembureau. Retrieved from https://cembureau.eu/policy-focus/sustainable-construction/#Sustainability\_standards.

Cembureau. (2015). EPD Ref: cemiii for CEM III by cembureau. Retrieved from https://cembureau.eu/policy-focus/sustainable-construction/#Sustainability\_standards.

CemSuisse. (2016). EPD Ref: Average Swiss Cement for Average Swiss Cement by Cemsuisse. Retrieved from https://www.cemsuisse.ch/umweltdeklarationen/?lang=de.

CemSuisse. (2016). EPD Ref: Swiss CEM I for Average Swiss CEM I by Cemsuisse. Retrieved from https://www.cemsuisse.ch/umweltdeklarationen/?lang=de.

CemSuisse. (2016). EPD Ref: Swiss CEM II/A for Average Swiss CEM II/A by Cemsuisse. Retrieved from https://www.cemsuisse.ch/umweltdeklarationen/?lang=de.

CemSuisse. (2016). EPD Ref: Swiss CEM II/B for Average Swiss CEM II/B by Cemsuisse. Retrieved from https://www.cemsuisse.ch/umweltdeklarationen/?lang=de.

CSA. (2016). EPD Ref: Portland limestone (GUL) cmeents for Portland limestone (GUL) cement by Cement Association of Canada. Retrieved from https://www.csaregistries.ca/epd/epd\_listing\_e.cfm.

CSA. (2016). EPD Ref: General use cement for General use (GU) cement by Cement Association of Canada. Retrieved from https://www.csaregistries.ca/epd/epd\_listing\_e.cfm.

DAPcons. (2017). EPD Ref: 100-001 for CEM I by Elite Cement. Retrieved from https://www.csostenible.net/dapcons/productes\_registrats?filtre=data&locale=en&validesa=false.

DAPcons. (2017). EPD Ref: 100-002 for Elite CEM II (ES) by Elite Cement. Retrieved from https://www.csostenible.net/dapcons/productes\_registrats?filtre=data&locale=en&validesa=false.

EPD Australasia. (2019). EPD Ref: S-P-01170 for GP Cement by Golden Bay Cement. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2019). EPD Ref: S-P-01170 for HP Cement by Golden Bay Cement. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2019). EPD Ref: S-P-00850 for GP Cement by Holcim. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2019). EPD Ref: S-P-00850 for GP Cement by Holcim. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Italia. (2017). EPD Ref: EPDitaly 0025 for Cement - CEM I by Buzzi Unicem. Retrieved from https://www.epditaly.it/en/view-view-epd/.

EPD Italia. (2017). EPD Ref: EPDitaly 0025 for Buzzi Unicem CEM II (IT) by Buzzi Unicem. Retrieved from https://www.epditaly.it/en/view-view-epd/.

EPD Italia. (2017). EPD Ref: EPDitaly 0025 for Cement - CEM IV by Buzzi Unicem. Retrieved from https://www.epditaly.it/en/view-view-epd/.

EPD Italia. (2017). EPD Ref: EPDitaly 0027 for Binder - average product by Buzzi Unicem. Retrieved from https://www.epditaly.it/en/view-view-epd/.

EPD Italia. (2017). EPD Ref: EPDitaly 0027 for Binder - Legante C.S.A. by Buzzi Unicem. Retrieved from https://www.epditaly.it/en/view-view-epd/.

EPD Norge. (2018). EPD Ref: NED-1539-528-NO for CEM I 52.5R Rapid cement by Cemex. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2015). EPD Ref: NEPD-1217-383-NO for CEM I, Fixed Cement (CEM I 52.5N) by Norcem. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2018). EPD Ref: NEPD-1483-489-NO for CEM I, Industrial Cement (52.5R) by Norcem. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2015). EPD Ref: NEPD-1217-383-NO for CEM I, Industrial Cement (52.5R) and Standard Cement (CEM I 42.5R) by Norcem. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2017). EPD Ref: NEDP-1426-468-EN for Rapid cement CEM I 52.5 N (LA) by Aalborg Portland. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2018). EPD Ref: NEPD-1545-531-NO for Cemex CEM II/B-S 52,5 N (DE) by Cemex. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2014). EPD Ref: NEPD00159E for Cemex CEM II/A-M (S-LL) 52,5 N (DE) by Cemex. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2017). EPD Ref: NEDP-1419-466-EN for Aalborg BASIS CEM II/A-LL 52.5 R (LA) (DK) by Aalborg Portland. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2016). EPD Ref: NEPD-1195-357-NO for Norcem FA CEM II/B-M (NO) by Norcem. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2015). EPD Ref: NEPD-24-201-NP updated for Norcem FA CEM II/A-V (NO) by Norcem. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2015). EPD Ref: NEPD-24-201-NP updated for Norcem FA CEM II/B-M (NO) by Norcem. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2015). EPD Ref: NEPD-211-199-NO for Norcem CEM II/B-M (NO) by Norcem. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2016). EPD Ref: NEPD-1199-371-NO for Cem III/A 42,5 L-LH/NA by Cemex. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2015). EPD Ref: NEPD00297E for Low-heat cement (Cem III / B 42.5 N-SR / LH // NA) by Cemex. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2018). EPD Ref: NEPD-1561-598-NO for Low-heat cement CEM III/B 42,5 L-LH/SR (na) by Cemex. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2015). EPD Ref: NEPD-359-235-EN for White cement, CEM I 52.5 R by Cemex. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2017). EPD Ref: NEPD-1418-467-EN for LOW ALKALI SULPHATE RESISTANT CEMENT by Aalborg Portland. Retrieved from https://www.epd-norge.no/sement/category324.html.

EPD Norge. (2013). EPD Ref: 00151N rev1 for Low carbon cement by Norcem. Retrieved from https://www.epd-norge.no/sement/category324.html.

GlobalEPD. (2014). EPD Ref: 003-001-rev 1 for Average Spanish CEM I by Oficement and IECA. Retrieved from https://www.aenor.com/certificacion/certificacion-de-producto/declaraciones-ambientales-de-producto/declaraciones-globalepd-en-vigor#des\_3.

GlobalEPD. (2014). EPD Ref: 003-002 rev 1 for Average Spanish CEM II by Oficement and IECA. Retrieved from https://www.aenor.com/certificacion/certificacion-de-producto/declaraciones-ambientales-de-producto/declaraciones-globalepd-en-vigor#des\_3.

GlobalEPD. (2014). EPD Ref: 003-003 for CEM III by Oficement and IECA. Retrieved from https://www.aenor.com/certificacion/certificacion-de-producto/declaraciones-ambientales-de-producto/declaraciones-globalepd-en-vigor#des\_3.

GlobalEPD. (2014). EPD Ref: 003-004-rev 1 for CEM IV by Oficement and IECA. Retrieved from https://www.aenor.com/certificacion/certificacion-de-producto/declaraciones-ambientales-de-producto/declaraciones-globalepd-en-vigor#des\_3.

GlobalEPD. (2014). EPD Ref: 003-005 for CEM V by Oficement and IECA. Retrieved from https://www.aenor.com/certificacion/certificacion-de-producto/declaraciones-ambientales-de-producto/declaraciones-globalepd-en-vigor#des\_3.

GlobalEPD. (2014). EPD Ref: 003-007 for Typical white cement type II by Oficement and IECA. Retrieved from https://www.aenor.com/certificacion/certificacion-de-producto/declaraciones-ambientales-de-producto/declaraciones-globalepd-en-vigor#des\_3.

GlobalEPD. (2014). EPD Ref: 003-006 for White cement type I by Oficement and IECA. Retrieved from https://www.aenor.com/certificacion/certificacion-de-producto/declaraciones-ambientales-de-producto/declaraciones-globalepd-en-vigor#des\_3.

IBU. (2014). EPD Ref: EPD-VÖZ-20140041-IAG1-DE for Average Austrian cement by Vereinigung der Österreichischen Zementindustrie. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2017). EPD Ref: EPD-VDZ-20170026-IAG1-DE for Average German cement by VDZ. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2017). EPD Ref: EPD-MPA-20170159-CAG1-EN for Average portland cement by Mineral Products Association. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2016). EPD Ref: EPD-HCG-20160145-CAD1-EN for CEM 1 52.5 R (rs) by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2014). EPD Ref: EPD-HCG-20140186-CAD1-EN for CEM I 42.5 N-SR 3/MH/LA by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2014). EPD Ref: EPD-HCG-20140187-CAD1-EN for CEM I 52.5 R by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-SIA-20140250-CAA1-EN for Portland cement CEM I 42.5 R by Sia CEMEX. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-SIA-20140249-CAA1-EN for Portland cement CEM I 52.5 R by Sia CEMEX. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2014). EPD Ref: EPD-HCG-20140235-CAD1-EN for Cementa CEM II/A-V 42.5 N (SE) by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2014). EPD Ref: EPD-HCG-20140205-CAA1-EN for Cementa CEM II/A-V 52.5 N (SE) by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2016). EPD Ref: EPD-CEM-20160146-CAA1-EN for Cemex Sia CEM II/A-M (S-LL) 52.5 N (LV) by Cemex. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2016). EPD Ref: EPD-HCG-20160235-CAD1-EN for Cementa Microfine CEM II/A-V 52.5 N (SE) by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-CIS-20150243-CAA1-EN for White portland cement CEM I 52.5 R by Cimsa. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-CIS-20150242-CAA1-EN for Cimsa ISADAC40 Calcium Aluminate cement by Cimsa. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-CIS-20160029-CAA1-EN for Cimsa RECIPRO40 Calcium Aluminate cement by Cimsa. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-CIS-20160031-CAA1-EN for Cimsa REFRO40 Calcium Aluminate cement by Cimsa. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-CIS-20160030-CAA1-EN for Cimsa RESISTO40 Calcium Aluminate cement by Cimsa. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2016). EPD Ref: EPD-HCG-20160236-CAD1-EN for Multicem by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2019). EPD Ref: EPD-HCG-20190046-CAA1-EN for CEM I by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2019). EPD Ref: EPD-HCG-20190047-CAA1-EN for CEM I by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2019). EPD Ref: EPD-HCG-20190140-CAA1-EN for CEM I by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2019). EPD Ref: EPD-HCG-20190141-CAA1-EN for CEM I by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2019). EPD Ref: EPD-HCG-20190045-CAA1-EN for Cementa CEM II/A-LL 42.5 R (SE) by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2019). EPD Ref: EPD-HCG-20190142-CAA1-EN for Cementa CEM II/A-V 52.5 N (SE) by Cementa AB. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2019). EPD Ref: EPD-HOI-20190109-IAA1-DE for Cementa CEM III/B 42.5 L-LH/SR (SE) by Holcim. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2016). EPD Ref: EPD-HGC-20160237-CAD1-EN for Portland fly ash cement CEM II/A-V 52.5N by Cementa. Retrieved from https://ibu-epd.com/en/published-epds/.

International EPD. (2018). EPD Ref: S-P-00404 for Ali CEM green by Italcementi. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2018). EPD Ref: S-P-00404 for Ali pre Green by Italcementi. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2014). EPD Ref: S-P-00523 for Portland cement - CEM I 52.5 N by Nesher Israel. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2014). EPD Ref: S-P-00524 for Nesher CEM II 42.5 N/B-LL (IS) by Nesher Israel. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2014). EPD Ref: S-P-00525 for Nesher CEM II 42.5 N/AM-SLV (IS) by Nesher Israel. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2014). EPD Ref: S-P-00527 for Average cement by Holcim Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00880 for Average Italian CEM I by AITEC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00880 for Average Italian CEM II by AITEC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00880 for Average Italian CEM III by AITEC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00880 for Average Italian CEM IV by AITEC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00895 for Votorantim CP II E 40 (slag) (BR) by Votorantim Cementos. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00895 for CP III-40 RS (Compound Portland cement from blast furnace sulphate resisting) by Votorantim Cementos. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00895 for CP V-ARI (Compound Portland cement with high early strength) by Votorantim Cementos. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2018). EPD Ref: S-P-01112 for Average Portland Pozzolana cement and Portland slag cement by ACC Ltd. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2018). EPD Ref: S-P-01113 for Average Portland Pozzolana cement by Ambuja. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2018). EPD Ref: S-P-01113 for Compocem by Ambuja. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2018). EPD Ref: S-P-01276 for Aalborg white cement CEM I 52.5R - SR5 (EA) by Aalborg Portland. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01414 for Portland slag cement by JSW Cement. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=12475&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

ITB. (2017). EPD Ref: 060/2017 for Hydraulic binder TEFRA 15 by Ekotech. Retrieved from https://www.itb.pl/epd.html#menu2.

MRPI. (2018). EPD Ref: 771 for Eco2cem cement by Ecocem. Retrieved from http://www.mrpi.nl/epd-certificaten.

MRPI. (2013). EPD Ref: 20.1.00027.005 for Fly ash by Vlieganasunie BV. Retrieved from http://www.mrpi.nl/epd-certificaten.

MRPI. (2013). EPD Ref: 20.1.00028.005 for Bottom ash by Vlieganasunie BV. Retrieved from http://www.mrpi.nl/epd-certificaten.

NRMCA. (2015). EPD Ref: NRMCAEPD:10008 for Type I cement by Capitol Aggregates. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: NRMCAEPD:10011 for Riverside cement - Plastic cement by CalPortland - Oro Grande plant. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: NRMCAEPD:10011 for Type IL cement by CalPortland - Oro Grande plant. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: NRMCAEPD:10011 for Riverside cement Type III by CalPortland - Oro Grande plant. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: NRMCAEPD:10011 for Riverside cement Type I/II/V by CalPortland - Oro Grande plant. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: NRMCAEPD:10022 for Type I/II/V cement by CalPortland - Mojave plant. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

**Aggregate Product EPD**

ASTM. (2017). EPD Ref: EPD 059 for #57 1" gravel by Polaris Materials Corporation. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 059 for #7 1/2" gravel by Polaris Materials Corporation. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 059 for WCS washed sand by Polaris Materials Corporation. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Drennan Yard: #6 stone by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Drennan Yard: #7 stone by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Parkdale: #6 stone by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Parkdale: #7 stone by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Riverbend facility: SQUEEGE 3/8 by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Riverbend facility: #89 RM blend by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Spanish Springs: 3/4 conc st by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Spanish Springs: 8stone by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Spanish Springs: AC 7/8 by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Specifications Aggregates 57/67 crushed rock by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Granite Canyon: 3/4 asphalt ST by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Granite Canyon: 57/67M/KDOTPCCM by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Granite Canyon:NB 47-B CO by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Drennan Yard: #67 washed rock by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Drennan Yard: 57/67 washed rock by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Parkdale: #67 washed rock by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Parkdale: 57 washed by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Parkdale: 57/67 washed rock by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Riverbend facility: 1-1/2 washed by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Riverbend facility: 57/67 washed rock by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Specifications Aggregates 57/67 crushed rock washed by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Riverbend facility: CLS 6 Recycled concrete base by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Drennan Yard: C-33 CONC SAND by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Parkdale: C-33 CONC SAND by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Riverbend facility: 3/18" pea gravel by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 063 for Riverbend facility: concrete sand ASTM 33 by Martin Marietta. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for 1" x #4 by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for 1/2" crushed by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for 3/4" crushed by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for 3/4" x #4 by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for 3/8" crushed by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for Class II base by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for Class II perm by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for Crushed class II PERM by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for Rock dust by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for MFG sand by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for pea gravel by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2017). EPD Ref: EPD 071 for Top sand by Vulcan. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 079 for 1 1/4 CSBC by Kangley Rock and Recycling. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 079 for 2" minus recycled gravel barrow by Kangley Rock and Recycling. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 079 for 2" x 3/4 RC ballast by Kangley Rock and Recycling. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 079 for 2" x 4" by Kangley Rock and Recycling. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 079 for 4" x 8" by Kangley Rock and Recycling. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 079 for 5/8" crushed (CSTC) by Kangley Rock and Recycling. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 079 for ASTM 457 (1 1/2") reyccled) by Kangley Rock and Recycling. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

BRE. (2016). EPD Ref: EPD 000105 for Generic aggregate by Tarmac. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 0001999 for Limestone aggregate by Aggregate Industries. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000205 for Granite aggregate - Bardon Hill by Aggregate Industries. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000206 for Granite aggregate - Bardon Hill by Aggregate Industries. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

EPD Norge. (2017). EPD Ref: NEPD-1257-403-SE for Crushed rock: primary crush by Skanska. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2017). EPD Ref: NEPD-1257-403-SE for Crushed rock: secondary crush by Skanska. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2017). EPD Ref: NEPD-1257-403-SE for Crushed rock: tertiary crush by Skanska. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2017). EPD Ref: NEPD-1257-403-SE for Crushed rock: blasting by Skanska. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1537-527-EN for Crushed stone aggregate products: blasting by Franzefoss Pukk. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1537-527-EN for Crushed stone aggregate products: primary crush by Franzefoss Pukk. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1537-527-EN for Crushed stone aggregate products: secondary crush by Franzefoss Pukk. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1537-527-EN for Crushed stone aggregate products: tertiary crush by Franzefoss Pukk. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1601-631-NO for 100% crushed stone / crumb, without additives, unpackaged: blasting by Feiring. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1601-631-NO for 100% Crushed stone / crumb, without additives, unpackaged: primary crush by Feiring. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1601-631-NO for 100% Crushed stone / crumb, without additives, unpackaged: secondary crush by Feiring. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1601-631-NO for 100% Crushed stone / crumb, without additives, unpackaged: tertiary crush by Feiring. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1602-632-NO for Crushed rock: blasting by Feiring. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1602-632-NO for Crushed rock: primary crush by Feiring. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1602-632-NO for Crushed rock: secondary crush by Feiring. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

EPD Norge. (2018). EPD Ref: NEPD-1602-632-NO for Crushed rock: tertiary crush by Feiring. Retrieved from https://www.epd-norge.no/asfalt-og-pukk/category326.html.

FDES. (2017). EPD Ref: - for Treatment of waste at end of life by UNPG. Retrieved from https://www.base-inies.fr/iniesV4/dist/consultation.html.

FDES. (2017). EPD Ref: - for Recycled aggregate by UNPG. Retrieved from https://www.base-inies.fr/iniesV4/dist/consultation.html.

FDES. (2017). EPD Ref: Aggregate from loose rocks for Aggregate from loose rocks by UNPG. Retrieved from https://www.base-inies.fr/iniesV4/dist/consultation.html.

FDES. (2017). EPD Ref: Aggregate from massive rocks for Aggregate from massive rocks by UNPG. Retrieved from https://www.base-inies.fr/iniesV4/dist/consultation.html.

International EPD. (2014). EPD Ref: S-P-00528 for Average aggregate by Holcim Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00842 for 0/150mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00842 for 0/90 mm, 0/45 mm, 32/63mm, 0/8mm, 0/16mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00842 for 0/32 mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00842 for 0/4, 0/27, 11/16, 16/22, 0/2, 2/5, 4/8, 8/11, 0/4mm KK7, 4/8mm KK7, 8/11 mm KK7, 11/16mm KK7 by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00843 for Blasted rock by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00843 for 0/250mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00843 for 0/32 mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00843 for 0/150, 0/90mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00843 for 32/63, 0/16, 0/8, 0/5mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00843 for 16/22mm, 16/32mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00843 for 0/2mm, 2/5mm, 2/8mm, 5/8mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00843 for Washed 32/63 mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00843 for Washed 16/32mm by NCC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

NRMCA. (2018). EPD Ref: NRMCAEPD 10020 for Average aggregate from AR Wilson quarry by Graniterock. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: NRMCAEPD 10020 for Average sand and gravel aggregate from Southside by Graniterock. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

SUGB. (2018). EPD Ref: FSKB-2018-1-ECOINVENT for Crushed natural aggregate 0/4 mm by ASAC. Retrieved from https://www.sugb.ch/dienstleistungen/umweltproduktedeklaration-epd/.

SUGB. (2018). EPD Ref: FSKB-2018-1-ECOINVENT for Natural aggregate 4/x mm, crushed by ASAC. Retrieved from https://www.sugb.ch/dienstleistungen/umweltproduktedeklaration-epd/.

SUGB. (2018). EPD Ref: FSKB-2018-1-ECOINVENT for Crushed recycled aggregate 0/x mm by ASAC. Retrieved from https://www.sugb.ch/dienstleistungen/umweltproduktedeklaration-epd/.

SUGB. (2018). EPD Ref: FSKB-2018-1-ECOINVENT for Round natural aggregate 0/4 mm by ASAC. Retrieved from https://www.sugb.ch/dienstleistungen/umweltproduktedeklaration-epd/.

SUGB. (2018). EPD Ref: FSKB-2018-1-ECOINVENT for Round natural aggregate 4/x mm by ASAC. Retrieved from https://www.sugb.ch/dienstleistungen/umweltproduktedeklaration-epd/.

**Specialist Aggregate Product EPD**

IBU. (2018). EPD Ref: EPD-BLV-20150064-IAD1-DE for Expanded clay aggregate by Bundesverband Leichtbeton. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-MIS-20150020-IAA2-DE for Misapor Schaumglas by Misapor. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2017). EPD Ref: EPD-XEL-20170148-IAD1-DE for Ytong granulate by Xella Baustoffe. Retrieved from https://ibu-epd.com/en/published-epds/.

International EPD. (2016). EPD Ref: S-P-00426 for Sand matrix® 0-2mm by Officina Dell'Ambiente. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00426 for Sand matrix® 0-4mm by Officina Dell'Ambiente. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00426 for Sand matrix® 2-4mm by Officina Dell'Ambiente. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00427 for AG matrix® by Officina Dell'Ambiente. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01088 for Foam glass 10-60mm by Hasopor. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

RT EPD. (2017). EPD Ref: RT EPD 007 for Expanded clay aggregate by LECA. Retrieved from https://cer.rts.fi/epd-ymparistoseloste/selaa-epd-ymparistoselosteita/.

**Admixture EPD**

IBU. (2017). EPD Ref: EPD-BAS-20170089-IBC1-EN for Master X-Seed by BASF. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2014). EPD Ref: EPD-DBC-20140005-IAE1-EN for Plasticiser and superplasticiser by Deutsche Bauchemie. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2014). EPD Ref: EPD-DBC-20140006-IAE1-EN for Water resisting admixtures by Deutsche Bauchemie. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2014). EPD Ref: EPD-DBC-20140007-IAE1-EN for Hardening accelerator by Deutsche Bauchemie. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2014). EPD Ref: EPD-DBC-20140008-IAE1-EN for Retarder by Deutsche Bauchemie. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2014). EPD Ref: EPD-DBC-20140009-IAE1-EN for Set Accelerator by Deutsche Bauchemie. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2014). EPD Ref: EPD-DBC-20140010-IAE1-EN for Air entrainer by Deutsche Bauchemie. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-EFC-20150086-IAG1-EN for Air entrainer by EFCA. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-EFC-20150087-IAG1-EN for Set Accelerator by EFCA. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-EFC-20150088-IAG1-EN for Retarder by EFCA. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-EFC-20150089-IAG1-EN for Hardening accelerator (3) by EFCA. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-EFC-20150090-IAG2-EN for Water resisting admixtures by EFCA. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2015). EPD Ref: EPD-EFC-20150091-IAG1-EN for plasticiser and superplasticiser by EFCA. Retrieved from https://ibu-epd.com/en/published-epds/.

International EPD. (2017). EPD Ref: S-P-01013 for Expancrete in 1000 kg bigbag (powder) by Mapei. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15362&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01013 for Mapecrete SRA-25 in 1000 litre IBC tank by Mapei. Retrieved from https://www.environdec.com/EPD-Search/.

International EPD. (2017). EPD Ref: S-P-01013 for Mapecrete SRA-N in 1000 litre IBC tank by Mapei. Retrieved from https://www.environdec.com/EPD-Search/.

**Ready Mix Concrete Product EPD**

ASTM. (2018). EPD Ref: EPD 083 for C15/20 by Emirates Beton. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 083 for C32/40 by Emirates Beton. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 083 for C36/45 by Emirates Beton. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 083 for C40/50 by Emirates Beton. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 083 for C40/50 by Emirates Beton. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

ASTM. (2018). EPD Ref: EPD 083 for C50/60 by Emirates Beton. Retrieved from https://www.astm.org/CERTIFICATION/EpdAndPCRs.html.

BRE. (2016). EPD Ref: EPD 000104 for Ready mix concrete by Tarmac. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2016). EPD Ref: EPD 000106 for Topflow by Tarmac. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2016). EPD Ref: EPD 000107 for Topforce (fibre reinforced RM concrete) by Tarmac. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2017). EPD Ref: EPD 000154 for Average Ready mix concrete by CRH Ciment. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000189 for C28/35 CI Ready mix concrete by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000190 for C32/40 CEMI ready mix concrete by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000191 for GEN3 CEMI ready mix concrete by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000192 for C28/35 CIIIA ready mix concrete by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000193 for C32/40 CIIIA ready mix concrete by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000194 for GEN3 CIIIA by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000195 for C28/35 CIIIB by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000196 for C32/42 CIIIB ready mix concrete by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

BRE. (2018). EPD Ref: EPD 000197 for Average ready mix by Hanson. Retrieved from http://www.greenbooklive.com/search/scheme.jsp?id=260.

EPD Australasia. (2014). EPD Ref: S-P-00555 for 17.5 Mpa by Allied Concrete. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2014). EPD Ref: S-P-00555 for 20 Mpa by Allied Concrete. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2014). EPD Ref: S-P-00555 for 25 Mpa by Allied Concrete. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2014). EPD Ref: S-P-00555 for 30 Mpa by Allied Concrete. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2014). EPD Ref: S-P-00555 for 35 Mpa by Allied Concrete. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2014). EPD Ref: S-P-00555 for 40 Mpa by Allied Concrete. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2014). EPD Ref: S-P-00555 for 45 Mpa by Allied Concrete. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2014). EPD Ref: S-P-00555 for 50 Mpa by Allied Concrete. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Australasia. (2019). EPD Ref: S-P-01165 for 106 specific mixes by Holcim Australia. Retrieved from https://epd-australasia.com/epd-category/cement-building-limes/.

EPD Italy. (2017). EPD Ref: EPDITALY0024 for Concrete by Unical. Retrieved from https://www.epditaly.it/en/view-view-epd/.

EPD Italy. (2018). EPD Ref: EPDITALY0028 for Concrete Green 0317 by Travelling Greenline. Retrieved from https://www.epditaly.it/en/view-view-epd/.

EPD Norge. (2013). EPD Ref: NEPD 169N for B30 M60 <200mm by Sola Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2014). EPD Ref: NEPD00272N for B30 M60 <200mm by Voss Cement. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2014). EPD Ref: NEPD00283N for B20 M90 D22 205000 by Norbetong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2016). EPD Ref: NEPD-1191-358-NO for B30 M60 D22 sync 200 by Olen Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2016). EPD Ref: NEPD-1219-381-n0 for B30 M60 D16 sink 200 by Mona Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1249-402-no for B30 M60 22mm 200mm sink by Alltid Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1250-402 for B35 MF45 16mm 200mm sink by Alltid Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1251-402 for B35 M45 16mm 200mm sink by Alltid Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1252-402-no for B45 MF40 16mm 200 sink by Alltid Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1254-402-no for B30 M60 16mm 240 sink by Alltid Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1301-423-NO for B30 M60 low carbon A 180 sink by Skedsmo Beton. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1346-446-no for B30 M60 D22 200 sink by Nordfjord Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1347-446-no for B45 SV standard D22 200 sink by Nordfjord Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1348-448-NO for B45 MF45 SV-low heat <200 sink by Velde Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1370-452-NO for B20 M90 D22 sync 200 by Ribe Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1444-479-NP for B30 M60 22mm 200mm sink low carbon Kl. B by Vestfold Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2017). EPD Ref: NEPD-1471-490-NP for 7540 B45 SV-standard 22mm tilsi by Betong Ost. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2018). EPD Ref: NEPD-1486-491-no for B30 M60 CL 0,40 D16 40% RED Avd. Leira by Ryfoss Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2018). EPD Ref: NEPD-1487-500-no for B30 M60 by Unicon. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2018). EPD Ref: NEPD-1546-529-NO for B30 M60 D16 S4, Cl 0.10, by Storegga Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2018). EPD Ref: NEPD-1551-520-NO for B30 M60 D22 sink 200 by Nordland Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2013). EPD Ref: NEPD-172N for B30 M60 180 by Skedsmo Beton. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2015). EPD Ref: NEPD-304-184-NO for B45 M40 Low heat concrete, sink 200mm by Skedsmo Beton. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2015). EPD Ref: NEPD-328-210-NO for B30 M60 <200 by Velde Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2015). EPD Ref: NEPD-332-216-no for B35 M45 <200 by Velde Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2015). EPD Ref: NEPD-333-217 for B45 M40 <200mm by Velde Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2015). EPD Ref: NEPD-334-218-NO for B45 SV40 <200mm by Velde Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2015). EPD Ref: NEPD-344-234-NP for B30 M60 D22 sink 180 by Sandnes & Jaerbetong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2016). EPD Ref: NEPD-389-275-NO for B30 M60 D22 by Berg Betong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

EPD Norge. (2016). EPD Ref: NEPD-421-291-NO for B30 M60 D22 sync 200 (Avd. Naerbo) by Sandnes & Jaerbetong. Retrieved from https://www.epd-norge.no/ferdig-betong/category317.html.

FDES. (2018). EPD Ref: 2-126:2019 for C16/20 X0 CEM II/A-S. by Syndicat National du Beton Pret a l’Emploi. Retrieved from https://www.base-inies.fr/iniesV4/dist/consultation.html.

FDES. (2018). EPD Ref: 2-127:2019 for C25/30 XC2 CEM II/A-L ou LL by Syndicat National du Beton Pret a l’Emploi. Retrieved from https://www.base-inies.fr/iniesV4/dist/consultation.html.

FDES. (2018). EPD Ref: 2-128:2019 for C2025 X0 CEM IIA by Syndicat National du Beton Pret a l’Emploi. Retrieved from https://www.base-inies.fr/iniesV4/dist/consultation.html.

IBU. (2016). EPD Ref: EPD-BAS-20160040-CAA1-EN for Diamondcrete by Aggregate Industries. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2016). EPD Ref: EPD-BAS-20160227-CAA1-EN for Watertight RMC by Aggregate Industries. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2017). EPD Ref: EPD-BAS-20170093-CAA1-EN for Agilia RMC by Aggregate Industries. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2018). EPD Ref: EPDIZB20180097IBG1DE for C20/25 by Federal Association of the German Transport Concrete Industry e.V. and the Research Association of the German Concrete and Precast Industry e.V.. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2018). EPD Ref: EPDIZB20180098IBG1DE for C35/45 by Federal Association of the German Transport Concrete Industry e.V. and the Research Association of the German Concrete and Precast Industry e.V.. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2018). EPD Ref: EPDIZB20180098IBG1DE for C45/55 by Federal Association of the German Transport Concrete Industry e.V. and the Research Association of the German Concrete and Precast Industry e.V.. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2018). EPD Ref: EPDIZB20180100IBG1DE for C50/60 by Federal Association of the German Transport Concrete Industry e.V. and the Research Association of the German Concrete and Precast Industry e.V.. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2018). EPD Ref: EPDIZB20180101IBG1DE for C25-30 by Federal Association of the German Transport Concrete Industry e.V. and the Research Association of the German Concrete and Precast Industry e.V.. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2018). EPD Ref: EPDIZB20180102IBG1DE for C30/37 by Federal Association of the German Transport Concrete Industry e.V. and the Research Association of the German Concrete and Precast Industry e.V.. Retrieved from https://ibu-epd.com/en/published-epds/.

IBU. (2018). EPD Ref: EPD-RMC-20180095 for C30/37 by BRMCA. Retrieved from https://ibu-epd.com/en/published-epds/.

International EPD. (2017). EPD Ref: S-P-00499 for Grey i.idro DRAIN by Italcementi. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-00499 for White i.idro DRAIN by Italcementi. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2014). EPD Ref: S-P-00526 for Average ready mix by Holcim Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2016). EPD Ref: S-P-00896 for FCK 30 MPA BR.1 ABAT 10+-2 by Votorantim Cimentos. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01018 for FCK 55 Mpa by Acciona. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2018). EPD Ref: S-P-01116 for Average ready mix by ACC. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for BCR 3.5 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for BCR 4 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for BCR 4.5 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for BCR 5 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C12/15 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C12/15 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C16/20 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C16/20 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C20/25 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C20/25 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C25/30 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C25/30 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C30/37 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C35/45 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C40/50 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C8/10 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01146 for C8/10 by General Beton Romania. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01203 for Grey i.idro DRAIN by Calcestruzzi. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2017). EPD Ref: S-P-01203 for White i.idro DRAIN by Calcestruzzi. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2018). EPD Ref: S-P-01209 for Average ready mix by Unibeton Readymix. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01624 for D06409 C40/50 50 by Transgulf. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01624 for D06535 C50/60 60 by Transgulf. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01624 for D06889 C50/60 60 by Transgulf. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01624 for D07375 C50/60 60 by Transgulf. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01624 for D07570 C50/60 60 by Transgulf. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01624 for D07571 C50/60 60 by Transgulf. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01624 for D07573 C50/60 60 by Transgulf. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01624 for D07988 C50/60 60 by Transgulf. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01624 for D08491 C50/60 60 by Transgulf. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01624 for D08672 C70/85 85 by Transgulf. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01629 for 12528 C35/20 cyl | C45/20 cube (50% OPC + 50%GGBS) by Quickmix. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01629 for 12529 C14/20 cyl | C18/20 cube (64% OPC + 36%GGBS) by Quickmix. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01629 for C35/20 cyl | C45/20 cube (45% OPC + 50%GGBS + 5% MS) by Quickmix. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

International EPD. (2019). EPD Ref: S-P-01722 for GO25 (10)-20-12-28-B by Cementos Bio Bio. Retrieved from https://www.environdec.com/EPD-Search/?search\_type=advanced&query=&country=&category=15363&certEpd=false&deregEpd=false&sectorEPD=false&ecoPlatformEPD=false&en15804EPD=false.

NRMCA. (2014). EPD Ref: 10004 for 19 mixes at 18 plants by Argos Ready Mix. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2014). EPD Ref: 10005 for 10014375 4000 psi by Argos Panama. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2014). EPD Ref: 10005 for 10019170 800 psi by Argos Panama. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10006 for 38 mixes by Graniterock. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for DOT,35,REG,2,6,T1,520,CLASS by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for DOT,35,REG,2,6,T1A20,517,CLASS by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for DOT,CLASS, AA by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,00,FF,8,6,T1A50,400 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,30,REG,LS,5,2,T1A25,440 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,30,REG,LS,5,5.5,T1A25,440 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,35,REG,LS,5,2,T1A20,470 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,35,REG,LS,5,2,T1A25,470 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,35,REG,LS,5,5.5,T1A25,470 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,35,REG,LS,5,6,T1A20,470 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,40,PRP,LS,7,2,T1A30,600 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,40,REG,LS,5,2,T1,520 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,40,REG,LS,5,2,T1A20,520 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,40,REG,LS,5,2,T1A25,520 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,40,REG,LS,5,5.5,T1A20,520 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,40,REG,LS5,5.5,T1A25,520 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,45,REG,LS,5,2,T1,570 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,45,REG,LS,5,2,T1A20,565,AG6 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,45,REG,LS,5,2,T1A25,565 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,45,REG,LS,5,2,T1A25,565,AG6 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,45,REG,LS,5,2,TA20,565 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,45,REG,LS,5,5.5,T1A25,565 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,45,REG,LS,5,6,TA20,565 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,50,REG,LS,5,2,T1,615 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,50,REG,LS,5,2,T1A20,615 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,50,REG,LS,5,5,T1,615 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,50,REG,LS,5,5,T1A20,615 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,55,REG,LS,5,2,T1A20,660 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,55,REG,LS,5,6,T1A20,660 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2015). EPD Ref: 10007 for SUB,60,REG,LS,5,2,T1A20,725 by GCC. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10010 for Exterio 3000 psi by Martin Marietta. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10012 for 30 mixes by Cemex Mexico - Armas. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10013 for 30 mixes by Cemex Mexico. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10014 for 30 mixes by Cemex Mexico - Juan Diaz. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10015 for 300h7400 by Concrete Supply Co. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10016 for 20GAOGBP by Golden Readymix. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10016 for 25GAOGBO1 by Golden Readymix. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10016 for 25GAOGBO2 by Golden Readymix. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10016 for 25GAS6 by Golden Readymix. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10016 for 30GAOGBO by Golden Readymix. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10016 for 40GAOGBO1 by Golden Readymix. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10016 for 40GAOGBO2 by Golden Readymix. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10016 for 40GAsA1 by Golden Readymix. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10016 for Screeds2 by Golden Readymix. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C30 - C35 (66%GGBS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C40 (36%GGBS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C40 (66%GGBS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C45 (36%GGBS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C45 (66%GGBS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C50 (36%GGBS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C55 ( 26%GGBS+5%MS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C60 (26%GGBS+5%MS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C65 (26%GGBS+6%MS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C70 (26%GGBS+7%MS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C75 (26%GGBS+7%MS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C80 (26%GGBS+8%MS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10017 for C90 (26%GGBS+8%MS) by Plants in Dubai Municipality. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2017). EPD Ref: 10018 for 30 mixes at 12 plants by CalPortland. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10019 for 50 mixes at 3 plants by CalPortland. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10021 for 30 mixes at 3 plants by Maschmeyer. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10023 for 171 products by Knife River. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C16/20 66% GGBS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C16/20 OPC + 36% GGBS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C16/20 OPC +66% GGBS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C20/10 OPC +66%GGBS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C25/20 OPC +66 GGBS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C35/45-s OPC +50% GGBS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C40/50 OPC + 60% GGBS +4% MS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C45/45-f OPC +66% GGBS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C50/20 OPC +66% GGBS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C50/60 OPC + 60% GGBS +5.4% MS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for c50/60-F OPC +65% GGBS +6% MS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for c50/60-S OPC +35%GGBS +5.4% MS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for c60/75 OPC + 65%GGBS +7.3%MS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for C60/75 OPC + 65%GGBS +9% MS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10024 for Type A&B C20/20 OPC + 36%GGBS by Austrian Arabian. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2018). EPD Ref: 10025 for 3000 Air entrained by Ready Mix USA. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NRMCA. (2019). EPD Ref: 20026 for 30 mixes at 9 plants by CalPortland. Retrieved from https://www.nrmca.org/sustainability/epdprogram/Index.asp.

NSF. (2013). EPD Ref: 10007 for 3000 psi concrete by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2013). EPD Ref: 10008 for 3000 psi concrete by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2013). EPD Ref: 10009 for 4000 psi concrete by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2013). EPD Ref: 10010 for 4000 psi concrete by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2013). EPD Ref: 10011 for 5000 psi concrete by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2013). EPD Ref: 10012 for 5000 psi concrete by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2013). EPD Ref: 10013 for 5000 psi concrete by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2013). EPD Ref: 10014 for 6000 psi concrete by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2013). EPD Ref: 10015 for 4000 psi concrete by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2013). EPD Ref: 10016 for 4500 psi concrete by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10018 for 5000 psi @56 days by Titan. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2013). EPD Ref: 10019 for 6000 psi concrete by Argos Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10020 for 4000 psi @ 56 days by Argos Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10028 for 4000 psi concrete by Redi-mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10033 for 24 MPa concrete by Redi-mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10034 for 24 MPa concrete by Redi-mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10035 for 24 MPa concrete by Redi-mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10036 for 24 MPa concrete by Redi-mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10037 for 24 MPa concrete by Redi-mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10071 for 24 MPa concrete by Redi-mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10072 for 24 MPa concrete by Redi-mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2014). EPD Ref: 10073 for 24 MPa concrete by Redi-mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 0-17.24 MPa, >20% FA and >30% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 0-17.24 MPa, >50% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 0-17.24 MPa, 0-19% FA/SL by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 0-17.24 MPa, 20-29% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 0-17.24 MPa, 30-39% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 0-17.24 MPa, 30-39% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 0-17.24 MPa, 40-49% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 0-17.24 MPa, 40-49% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 17.25-20.68 MPa, >20% FA and >30% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 17.25-20.68 MPa, >50% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 17.25-20.68 MPa, 0-19% FA/SL by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 17.25-20.68 MPa, 20-29% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 17.25-20.68 MPa, 30-39% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 17.25-20.68 MPa, 30-39% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 17.25-20.68 MPa, 40-49% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 17.25-20.68 MPa, 40-49% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 20.69-27.58 MPa, >20% FA and >30% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 20.69-27.58 MPa, >50% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 20.69-27.58 MPa, 0-19% FA/SL by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 20.69-27.58 MPa, 20-29% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 20.69-27.58 MPa, 30-39% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 20.69-27.58 MPa, 30-39% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 20.69-27.58 MPa, 40-49% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 20.69-27.58 MPa, 40-49% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 27.59-34.47 MPa, >20% FA and >30% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 27.59-34.47 MPa, >50% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 27.59-34.47 MPa, 0-19% FA/SL by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 27.59-34.47 MPa, 20-29% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 27.59-34.47 MPa, 30-39% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 27.59-34.47 MPa, 30-39% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 27.59-34.47 MPa, 40-49% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 27.59-34.47 MPa, 40-49% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 34.48-41.37 MPa, >20% FA and >30% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 34.48-41.37 MPa, >50% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 34.48-41.37 MPa, 0-19% FA/SL by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 34.48-41.37 MPa, 20-29% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 34.48-41.37 MPa, 30-39% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 34.48-41.37 MPa, 30-39% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 34.48-41.37 MPa, 40-49% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 34.48-41.37 MPa, 40-49% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 41.38-55.16 MPa, >20% FA and >30% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 41.38-55.16 MPa, >50% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 41.38-55.16 MPa, 0-19% FA/SL by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 41.38-55.16 MPa, 20-29% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 41.38-55.16 MPa, 30-39% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 41.38-55.16 MPa, 30-39% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 41.38-55.16 MPa, 40-49% FA by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10080 for 41.38-55.16 MPa, 40-49% slag by NRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10091 for 35 Mpa concrete by Comosa. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GU with air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GU with air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GU with air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GU with air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GU with air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GU without air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GU without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GU without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GU without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GU without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GUL with air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GUL with air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GUL with air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GUL with air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GUL without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GUL without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GUL without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 GUL without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 25 Industry Average Benchmark by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GU with air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GU with air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GU with air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GU with air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GU with air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GU without air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GU without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GU without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GU without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GU without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GUL with air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GUL with air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GUL with air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GUL with air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GUL without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GUL without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GUL without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 GUL without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 30 Industry Average Benchmark by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GU with air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GU with air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GU with air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GU with air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GU with air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GU without air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GU without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GU without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GU without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GU without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GUL with air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GUL with air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GUL with air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GUL with air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GUL without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GUL without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GUL without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 GUL without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 35 Industry Average Benchmark by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GU with air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GU with air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GU with air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GU with air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GU with air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GU without air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GU without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GU without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GU without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GU without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GUL with air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GUL with air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GUL with air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GUL with air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GUL without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GUL without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GUL without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 GUL without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 40 Industry Average Benchmark by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 45 GU without air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 45 GU without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 45 GU without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 45 GU without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 45 GU without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 45 GUL without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 45 GUL without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 45 GUL without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 45 GUL without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 45 Industry Average Benchmark by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GU with air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GU with air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GU with air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GU with air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GU with air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GU without air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GU without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GU without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GU without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GU without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GUL with air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GUL with air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GUL with air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GUL with air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GUL without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GUL without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GUL without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 GUL without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 50 Industry Average Benchmark by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 55 GU without air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 55 GU without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 55 GU without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 55 GU without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 55 GU without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 55 GUL without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 55 GUL without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 55 GUL without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 55 GUL without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 55 Industry Average Benchmark by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 60 GU without air 0-14% FA/SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 60 GU without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 60 GU without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 60 GU without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 60 GU without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 60 GUL without air 15-29% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 60 GUL without air 25-34% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 60 GUL without air 30-40% FA by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 60 GUL without air 35-50% SC by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2016). EPD Ref: 10092 for 60 Industry Average Benchmark by CRMCA. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10095 for 55 Mpa concrete by Concretos Cruz Azul. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10103 for 50-150 psi by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10104 for 100-300 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10105 for 4500 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10106 for 4500 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10107 for 5000 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10108 for 6500 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10109 for 350 kgf/m2 by Forzac. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10120 for 35 Mpa concrete by Concretos Cruz Azul. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10121 for 40 Mpa concrete by Concretos Cruz Azul. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10122 for 40 Mpa concrete by Concretos Cruz Azul. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10124 for 50-150 psi concrete by Service Rock Products. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10125 for 4500 psi concrete by Service Rock Products. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10126 for 4500 psi concrete by Service Rock Products. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10127 for 5000 psi concrete by Service Rock Products. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10128 for 6500 psi concrete by Service Rock Products. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10129 for 100-300 by Service Rock Products. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10130 for 35 Mpa concrete for precast by Sepsa. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10131 for 200 kgf/m2 by Forzac. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10143 for 5000 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10144 for 6000 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2017). EPD Ref: 10145 for 8000 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2018). EPD Ref: 10154 for 5000 psi concrete for Al Moosa hospital by HACO. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10159 for 1500 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10160 for 4500 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10161 for 4500 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10162 for 3500 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10163 for 5000 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10165 for 3000 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10165 for 6000 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10166 for 4000 psi concrete by Nevada Ready Mix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10238 for 31 Mpa concrete by Lauren. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10239 for 55 Mpa concrete by Lauren. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10240 for 41.4 Mpa by Lauren. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10241 for 34.5 Mpa by Lauren. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10242 for 31 Mpa by Lauren. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10243 for 24.1 by Lauren. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10244 for 44.4 by Lauren. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10255 for 50 Mpa concrete by Al Kifah. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10256 for 65 Mpa concrete by Saudi Readymix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10257 for 35 Mpa concrete by Saudi Readymix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10258 for 37 Mpa by Saudi Readymix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10259 for 50 Mpa concrete by Saudi Readymix. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10261 for 3000 psi concrete by Cadman. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10262 for 4000 psi concrete by Cadman. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10263 for 4000 psi concrete by Cadman. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10264 for 400 psi concrete by Cadman. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp.

NSF. (2019). EPD Ref: 10265 for 400 psi concrete by Cadman. Retrieved from http://info.nsf.org/Certified/Sustain/epd\_search.asp